|  |  |  |
| --- | --- | --- |
| **Student Name** | **Student Surname** | **Student ID** |
| Salvatore Gabriele | La Greca | S281589 |

A cartoon of a castle

Description automatically generated with medium confidenceA picture containing blue, dark

Description automatically generated

**SAVE THIS FILE IN PDF AND SUBMIT IT ON “EXERCISE”**

testing and fault tolerance

Laboratory Session 2: “ATPG & Fault Simulation”

# **[A] Fault Simulation of External Patterns**

The purpose of this exercise is to implement a tcl script that applies a fault simulation flow for the stuck-at fault model. TestMAX can then execute the script as follows:

* tmax your\_script.tcl -shell

TestMAX can simulate test patterns defined in different formats, such as in STIL (Standard Test Interface Language). Patterns stored in STIL files are compliant with the test procedures, which are also described in the same file and are read by TestMAX during the Design Rule Checking (DRC) process. As an example, the following code snippet shows two combinational patterns stored in a STIL file:

"pattern 0": Call "capture" { "\_pi"=10100; "\_po"=HLLHLHLHL; }

"pattern 1": Call "capture" { "\_pi"=11001; "\_po"=LHHHLHLHL; }

In the example, \_pi is follows by the values to be applied to the primary inputs, while \_po is followed by the values that are expected on the primary outputs when the patterns are applied.

**[A.1] Tasks:**

1. Check the contents of the STIL files in the folder and complete the table below
2. Create a TestMAX script for the fault simulation of the C6288 benchmark circuit by using the external test patterns stored in the STIL file. Add all stuck-at faults in the circuit while allowing the masking of some of the primary outputs (see [Appendix A: TestMAX Flow](#_Appendix_A:_TetraMAX)).

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Circuit** | **PIs** | **POs** | **Clock signals** | **Test patterns** |
| C6288 | datai(31..0) | datao(31..0) | - | 59 |
| b10 | 13 | 6 | clock | 0 |
| b12 | 7 | 6 | clock | 0 |

* In the DRC command mode it is possible to mask some of the primary outputs. This means that a fault effect propagated to such an output is not considered as detected by the fault simulator. PO masks are added during the DRC mode of the flow. For instance, if you want to mask all possible ports but two, you can do it via the following flow:
* DRC-T> add\_po\_masks -all
* DRC-T> remove\_po\_masks <output port 1 name>
* DRC-T> remove\_po\_masks <output port 2 name>
* It is possible to get the list of primary output pins and the current PO masks with the following commands:
* DRC-T> report\_primitives -pos
* DRC-T> report\_po\_masks

**[A.2] Tasks:**

1. Complete the following table by applying the proper PO masks to the C6288 circuit:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **PO Masks** | **Test patterns** | **Test coverage** | **Not controlled faults** | **Not observed faults** |
| *none* | 59 | 99.88% | 0 | 17 |
| datao(1) | 59 | 99.83% | 0 | 17 |
| datao(2) | 59 | 99.72% | 0 | 20 |
| datao(3) | 59 | 99.71% | 0 | 22 |
| datao(1) to datao(3) | 59 | 99.32% | 0 | 50 |
| all but datao(1) to datao(3) | 59 | 29.39% | 0 | 9671 |
| *all* | 59 | 0.00% | 0 | 6304 |

# **[B] Combinational ATPG**

In this exercise, TestMAX generates the patterns internally by means of the Automatic Test Pattern Generation (ATPG) process. As for the fault simulation, you can create a tcl script by following the guidelines in the figure. The script shall generate test patterns for a combinational circuit by using all stuck-at faults and allowing the masking of some primary outputs (as for the fault simulation script) and the application of constraints to some primary inputs (PIs).

You can use STIL procedures to force a constrained port to a state other than the requested constrained value for a limited number of tester cycles and then, return the port to its constrained value. For example, you might want to hold a global reset port to an off state for general ATPG patterns, but then allow it to be asserted to initialize the design. You can reproduce this behavior using TestMAX during the DRC phase, where it is possible to define constraints on the PIs as follows:

* DRC-T> add\_pi\_constraints 0 <port name> *# the pin is tied’0*
* DRC-T> add\_pi\_constraints 1 <port name> *# the pin is tied’1*
* DRC-T> add\_pi\_constraints x <port name> *# the pin is not controllable*

The command can be repeated for each primary input pin to be constrained. The list of primary inputs can be obtained as follows:

* DRC-T> report\_primitives –pis

Additionally, you can also define restrictions on internal signals, which are not possible to be constrained with the add\_pi\_constraints command. Such features are not needed for the purposes of this exercise and you can check the user manual if you are interested.

**[B.1] Tasks:**

1. Complete the following table after running the ATPG on the C6288 circuit, each time applying the requested primary input constraints and primary output masks while gathering the results from the TestMAX reports.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **PI Constraints** | **PO Masks** | **Test Patterns** | **Test coverage** | **ATPG Untestable faults** | **Aborted faults** |
| *none* | *none* | 36 | 100% | 0 | 0 |
| datai(0) = 0 | *none* | 36 | 98.72% | 186 | 0 |
| datai(0) = 1 | *none* | 35 | 99.85% | 22 | 0 |
| datai(1) = X | *none* | 58 | 95.49% | 394 | 128 |
| datai(0) to datai(2) = 0 | *none* | 35 | 95.41% | 620 | 45 |
| datai(0) to datai(2) = 1 | *none* | 36 | 99.47% | 76 | 0 |
| datai(0) to datai(2) = X | *none* | 66 | 90.67% | 1169 | 153 |
| datai(0) to datai(2) = X | datao(1) to datao(3) | 65 | 89.99% | 1279 | 128 |
| datai(0) to datai(2) = X | All but datao(1) to datao(3) | 1 | 0.77% | 2368 | 11724 |
| *none* | *all* | 0 | 0.00% | 9604 | 4871 |

# **[C] Full Sequential ATPG**

In case of sequential circuits, the ATPG process using the functional input and output pins of the circuit is performed in the so-called *Full Sequential Mode* (which is activated using the proper setting, as in the figure). Moreover, you need to define clocks and reset signals, either by means of a STIL file, or explicitly in the DRC mode.

**[C.1] Tasks:**

1. Complete the following table after running the full sequential ATPG on the b10 and b12 benchmarks, which are sequential circuits.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Circuit** | **Stuck-at faults** | **Test Patterns** | **Test coverage** | **Aborted faults** | **CPU time** |
| b10 | 1124 | 33 | 91.10% | 6 | 308.88 |
| b12 | 6168 | 13 | 14.49% | 4788 | 49830.24 |

* Since the process may require a lot of time (high complexity), it is possible to run it in background using[**byobu**](https://www.byobu.org/), an enhanced terminal multiplexer SW as follows:

1. Connect to the remote server and run byobuon the terminal
2. Run the TestMAX script in the byobu shell
3. Press **F6** to *detach* the byobu shell. Now you can disconnect from the remote server, the work will continue in background
4. When you connect again to the remote server, run again byobu and you will *attach* to the shell.

# **Appendix A: TestMAX Flow**

**BUILD-T>**

***Read the VHDL/Verilog library models and netlist:***

* read\_netlist <HDL file name> –library [-insensitive]
* read\_netlist <HDL file name> –master [-insensitive]

***Elaborate the top-level***

* run\_build\_model <top-level module name>

build

drc

**DRC-T>**

***Add clock/reset signals (not needed if you use an .spf file)***

* add\_clock <off-state value (01)> <signal name>

***Add Primary input constraints and output masks if needed***

* add\_pi\_constraints <01X value> <input port name>
* add\_po\_masks <output port name>

***Run default DRC or use .spf file***

* run\_drc [<SPF file name>]

*ATPG*

***Set fault model***

* set\_faults -model stuck

***Create fault list or import it (one of the following)***

* add\_faults -all
* add\_faults <instance name> **or** add\_faults -module <module name>
* read\_faults <file name> -add [-force\_retain\_code] [-maintain\_detection]
* run\_drc [<SPF file name>]

***Report summaries***

* set\_faults -summary verbose -fault\_coverage
* report\_summaries

***Write fault list***

* write\_faults <file name> -all -uncollapsed -replace

*Fault simulation*

**TEST-T>**

***Read external patterns***

* set\_patterns -external <STIL file>

***Check external patterns***

* run\_simulation [-sequential]

***Run fault simulation***

* run\_fault\_sim [-sequential]

***Select internal patterns***

* set\_patterns -internal

***Set ATPG options (check the manual)***

* set\_atpg -help **or** man set\_atpg

***For sequential circuits***

* set\_atpg -full\_seq\_atpg

***Run ATPG***

* run\_atpg -auto\_compression

Run ATPG

run\_atpg[-sequential]

## **Appendix B: Files of LAB2**

* **All files listed here are included in your remote /home directory under lab2 folder.**

|  |  |
| --- | --- |
| **Filename** | **Description** |
| b10.v | ITC’99 b10 netlist (sequential circuit) |
| b12.spf | ITC’99 b10 STIL procedure file |
| b12.v | ITC’99 b12 netlist (sequential circuit) |
| b12.spf | ITC’99 b12 STIL procedure file |
| c6288.vhd | ISCAS’85 c6288 netlist (combinational circuit) |
| c6288.stil | ISCAS’85 STIL procedure file and test patterns |
| pt2002.v | Technology library models |

# **Appendix C: Commands & Techniques**

## [C.i] Fault-free simulation

A fault-free (or *gold*) machine simulation using the external patterns should be performed before running a fault simulation, to compare the TestMAX simulation responses with the expected responses found in the patterns. If the gold machine simulation reports errors, there is little value in proceeding to run fault simulation.

The gold machine simulation can be performed with the following command:

* TEST-T> run\_simulation -sequential

In case of error, TestMAX reports a list of messages indicating the simulation mismatches, as in the following example:

* TEST-T> run\_simulation -sequential

Begin sequential simulation of 36 external patterns.

10 o\_y2 (exp=1, got=0)

20 o\_y10 (exp=1, got=0)

Simulation completed: #patterns=36/102, #fail\_pats=2(0), #failing\_meas=2(0)

## [C.ii] Fault Injection using TestMAX

The run\_simulation command can be used to perform a logic simulation of the current pattern source determined by the set\_patterns command and it reports any differences between simulated and expected values. This simulation can be performed in the presence of a selected fault and will report all failures that result from the fault.

After performing a fault-simulation, one fault marked as Detected by Simulation (DS) can be selected from the fault list and injected in the circuit.

For a logic defect, there are four types of fault behavior that you can select by means of the -stuck option: stuck-at-0 (0), stuck-at-1 (1), stuck-at-01 (01), and stuck-at-X (X). For the stuck-at-01 fault type, the value is fixed either to 0 or 1 for each pattern for all affected fanout branches. For the stuck-at-X fault type, the value is fixed either to 0 or 1 for each time frame for all affected fanout branches. All affected fanout branches have the same value.

The -stuck option supports multiple arguments of the same type. You can specify a maximum of ten logic faults for different pins, however only one injection is supported for a stuck-at-01 logic defect.

The following example simulates a single stuck-at-01 fault:

* TEST-T> run\_simulation -stuck { 01 ucore/freg/u540 }

The following example simulates a stuck-at-0 and a stuck-at-1 fault:

* TEST-T> run\_simulation -stuck { 0 ucore/freg/u540 1 ucore/alu/u27 }

Transition delay faults can also be injected in the circuit. The following example simulates a rising transition delay fault in functional logic:

* TEST-T> run\_simulation -slow { r ucore/freg/u540 }

## [B.iii] Modify STIL Patterns

The patterns stored in the STIL file contain both primary input and primary output values. It means that, if the primary input values are modified, the primary output values need to be modified accordingly. You can use TestMAX to simulate patterns on the fault-free circuit and to update the primary output values. The updated patterns can be written back into a STIL file, as in the following example:

* TEST-T> set\_patterns -external patterns*.stil*
* TEST-T> run\_simulation -sequential -update
* TEST-T> write\_patterns patterns\_update.stil -external –format stil

As an exercise, you can duplicate the C6288 STIL file and replace the \_pi signals of the original patterns with the following values:

01010101010101011111111111111111

10101010101010101111111111111111

01010101010101011101111111111111

10101010101010101101111111111111

11011011011011011111111111111111

01101101101101101111111111111111

10110110110110111111111111111111

11111111111111111101010101010101

11111111111111110110101010101010

11111111111111101101010101010101

11111111111111100110101010101010

11111111111111110000000000000000

Then, you can run the TestMAX script to update the POs accordingly, followed by a fault simulation to evaluate the new fault coverage.

## [B.iv] N-times Detection

When you run the ATPG and the fault simulation processes with the default options, TestMAX considers a fault as detected when a difference is propagated to an observable primary output. By using the N-times detection option (ndetects)*,* you can specify how many times a fault must be excited and propagated to an observable primary output before being considered as detected, as in the following examples:

* TEST-T> run\_fault\_sim –sequential –ndetects 5
* TEST-T> run\_atpg –auto\_compression –ndetects 5

As an exercise, you can play with the N-times detection option during the C6288 fault simulation and see how the fault coverage changes with respect to the one obtained in the first exercise. Moreover, you can do the same for the ATPG and compare the results with the previous exercises.

## [B.v] Incremental ATPG

Typically, the ATPG process may be iterated until a sufficient fault coverage is obtained. Especially for large designs, it may happen that the first execution of the ATPG process is quite ineffective. This is typically due to the default ATPG options, or to specific testing strategies.

For example, the first run may be executed by limiting the number of patterns to generate and trying to compact them as well as possible. This can be done as in the following example:

* TEST-T> set\_atpg -patterns 500 -merge high
* TEST-T> run\_atpg

At the end of an ATPG process, the new generated patterns are added to the internal pattern set, while the current fault list is updated. This means that a new ATPG process can be started on the current fault list.

Moreover, you can run an ATPG process after a fault simulation, as follows:

* TEST-T> set\_patterns –external patterns.stil
* TEST-T> run\_fault\_sim -sequential
* TEST-T> set\_patterns -internal
* TEST-T> run\_atpg

Another parameter which may impact on the effectiveness of the ATPG process is the *abort limit*. The search for a pattern by the ATPG algorithm involves making a decision and certain assumptions, setting inputs values, and determining whether controllability and observability can be attained. When an assumption is proved false or some restriction or blockage is encountered, the algorithm backs up, remakes the decision, and proceeds until the abort limit is reached or a pattern is found to detect the fault. The value of the *abort limit* parameter can be set as in the following example:

* TEST-T> set\_atpg –abort\_limit 20

By increasing the value of such a parameter, the process will require higher levels of effort. Determining an appropriate setting for the abort limit is an iterative process. The following example sequence shows how to play with this feature:

* TEST-T> set\_atpg -abort\_limit 10 -merge off
* TEST-T> run\_atpg
* TEST-T> set\_atpg -abort 50
* TEST-T> run\_atpg
* TEST-T> set\_atpg -abort 250
* TEST-T> run\_atpg

As an exercise, you can try to improve the fault coverage obtained in the ATPG of the C6288, especially with many PI constraints and PO masks, by acting on the abort limit value.